	
	
	
	Tost Winch Maintenance Schedule
	

	
	
	
	
	
	
	
	

	Daily (Driver inspection - see also Winch Driver's Manual)
	
	

	Check and top up if necessary, the following on both winch and road chassis

	
	Engine oil
	
	
	
	
	

	
	Auto transmission oil
	
	
	
	

	
	Radiator
	
	
	
	
	
	

	
	Fuel
	
	
	
	
	
	

	Check fan belt - condition and tension
	
	
	
	

	Check function of lights and gauges
	
	
	
	

	Check serviceability of paying on gear and guillotines
	
	

	Check tyres fully inflated
	
	
	
	
	

	
	
	
	
	
	
	
	

	Monthly
	
	
	
	
	
	
	

	Functional check of guillotines (without cutting cable) - BGA requirement

	Check paying on rollers - lubricate as necessary, replace damaged items
	

	
	
	
	
	
	
	
	

	Quarterly
	
	
	
	
	
	
	

	Check function of all gauges and warning lights
	
	
	

	Check setting and function of rev limiter
	
	
	
	

	Check fan belt - condition and tension
	
	
	
	

	Check and top up if required, the following on bothe winch and road chassis.

	
	Engine oil (change oil and filter if engine is in 'daily' use)
	

	
	Auto transmission oil
	
	
	
	

	
	Radiator
	
	
	
	
	
	

	
	Main gearbox
	
	
	
	
	

	
	Right angle drive/back axle
	
	
	
	

	
	Dog clutch housings
	
	
	
	
	

	
	Scroll gear housings
	
	
	
	
	

	
	Brake fluid
	
	
	
	
	

	
	Clutch fluid
	
	
	
	
	

	
	Batteries
	
	
	
	
	
	

	Investigate reasons for any significant topping up
	
	
	

	Lubricate paying on gear pivots
	
	
	
	

	Lubricate dog clutch selectors and linkage
	
	
	

	Check/adjust tyre pressures. Check for damage or wear.
	
	

	
	
	
	
	
	
	
	

	Half yearly
	
	
	
	
	
	

	Change auto transmission oil and filter
	
	
	
	

	
	
	
	
	
	
	
	

	Every autumn
	
	
	
	
	
	

	Inspect hoses - replace if cracked or leaking
	
	
	

	Check security of all hose clips
	
	
	
	
	

	Check fan belt - condition and tension
	
	
	
	

	Drain and refill cooling system with 30% (min) antif-freeze solution
	


